**Coaxial Cable to SMA Connector Printed Circuit Board Fabrication Information**

* Number of layers: 2
* Substrate: 0.062” FR4
* Board width: .5”
* Board height: .3”
* Board outline: Mechanical layer 1
* Copper weight: (not important)
* Surface: HASL or ENIG (not important)
* Board shape: Rectangle
* Cutouts: None
* Holes/Vias: None
* Solder mask color: Green (not important)
* Sinkscreen layers: top
* Sinkscreen color: White
* Electrical Test: Not required
* Routing: Either individual or panalized with v-scores

|  |  |
| --- | --- |
| **Top** | **Bottom** |
|  |  |